This folder contains the results of measurements of second harmonic hyper-Rayleigh scattering (SHRS) intensity as a function of the angle of an analysing polariser (analyser), which was placed in front of the detector.

HWP angle equal to 0 (specified in the file name) corresponds to incident S-polarised light.
HWP angle equal to 45 (specified in the file name) corresponds to incident P-polarised light.

The analyser angle is specified in the file name.

The second column of the text files contains SHRS intensity in counts/second.
The different rows correspond to individual measurements (repeats) with the same parameters.