
New TopShim run:

version = topshim 2.0.0
date = 2022-01-10
time = 18:28:09.963
command = topshim 

1D SHIMMING

Parameters:

maximum order = 5
probe = Z163739_0080
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm
optimisation parameters = ls
linewidth 1H = 0.10 Hz
envelope shape / strictness = 2.00 / 200

Results:

echo time must be reduced
initial B0 stdDev = 17.35 Hz
sample size = 2.53 cm, position = 0.20 cm
final B0 stdDev = 11.58 Hz > improvement = 1.5
envelope width = 2.46 Hz
shim changes: 
Z	-110
Z2	+12
Z3	-218
Z4	-220
Z5	+215

duration = 1 min 41 sec
completed successfully
finished Mon Jan 10 18:29:49 2022


========================================================================
