
New TopShim run:

version = topshim 2.0.0
date = 2022-01-10
time = 18:08:40.157
command = topshim 

1D SHIMMING

Parameters:

maximum order = 5
probe = Z163739_0080
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm
optimisation parameters = ls
linewidth 1H = 0.10 Hz
envelope shape / strictness = 2.00 / 200

Results:

initial B0 stdDev = 15.51 Hz
sample size = 2.45 cm, position = 0.19 cm
final B0 stdDev = 6.10 Hz > improvement = 2.5
envelope width = 3.24 Hz
shim changes: 
Z	-82
Z2	+37
Z3	-294
Z4	-473
Z5	+488

duration = 1 min 11 sec
completed successfully
finished Mon Jan 10 18:09:49 2022


========================================================================
