EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
T_NAME		Date_
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 50000000
		REL	"Date_=itodate(DATE)"
		INV_REL	"DATE=datetoi(Date_,DATE)"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		Time
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"Time=itotime(DATE)"
		INV_REL	"DATE=timetoi(Time,DATE)"
		FORMAT	"%14.2f h"
		TEXT	" "
END
NAME		INSTRUM
		TEXT	" "
END
NAME		PROBHD
		FORMAT	"%14.14s"
		TEXT	" "
END
NAME		PULPROG
		TEXT	" "
END
NAME		TD
		TEXT	" "
END
NAME		SOLVENT
		TEXT	" "
END
NAME		NS
		TEXT	" "
END
NAME		DS
		TEXT	" "
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e8
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.3f Hz"
		TEXT	" "
END
T_NAME          FIDRES
                TYPE    R32
                CLASS   ACQU
                SUBRANGE 0.0 100000
                REL     "FIDRES=2*SW*SFO1/TD"
                INV_REL "TD = nextpow(2*SW*SFO1/FIDRES)"
		UNIT	"Hz"
		FORMAT	"%14.6f Hz"
		TEXT	" "
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
		TEXT	" "
END
NAME		RG
		TEXT	" "
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3lf usec"
		TEXT	" "
END
NAME		DE
		FORMAT	"%14.2f usec"
		TEXT	" "
END
NAME		TE
		FORMAT	"%14.1f K"
		TEXT	" "
END
T_NAME		CNST6
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST6=CNST[6]"
INV_REL	"CNST[6]=CNST6"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST7
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST7=CNST[7]"
INV_REL	"CNST[7]=CNST7"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST13
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST13=CNST[13]"
INV_REL	"CNST[13]=CNST13"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		CNST30
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"CNST30=CNST[30]"
INV_REL	"CNST[30]=CNST30"
FORMAT	"%14.7f"
TEXT	" "
END
T_NAME		D0
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D0=D[0]"
INV_REL	"D[0]=D0"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D1=D[1]"
INV_REL	"D[1]=D1"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D6
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D6=D[6]"
INV_REL	"D[6]=D6"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		D16
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"D16=D[16]"
INV_REL	"D[16]=D16"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
T_NAME		IN0
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1e38
REL	"IN0=IN[0]"
INV_REL	"IN[0]=IN0"
UNIT	"sec"
FORMAT	"%14.8f sec"
TEXT	" "
END
NAME		TDav
		TEXT	" "
END
NAME		SFO1
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC1
NONEDIT
TEXT	" "
END
T_NAME		P1
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P1=P[1]"
INV_REL	"P[1]=P1"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P2
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P2=P[2]"
INV_REL	"P[2]=P2"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW1
TYPE	R32
CLASS	ACQU
REL	"PLW1=PLW[1]"
INV_REL	"PLW[1]=PLW1"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW1 "
END
NAME		SFO2
FORMAT	"%14.7f MHz"
TEXT	" "
END
NAME		NUC2
NONEDIT
TEXT	" "
END
T_NAME		P3
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P3=P[3]"
INV_REL	"P[3]=P3"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		P24
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P24=P[24]"
INV_REL	"P[24]=P24"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
T_NAME		PLW2
TYPE	R32
CLASS	ACQU
REL	"PLW2=PLW[2]"
INV_REL	"PLW[2]=PLW2"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"power PLW2 "
END
NAME		SPNAM[7]
TEXT	" "
END
T_NAME		SPOAL7
TYPE	R32
CLASS	ACQU
SUBRANGE -1.0 1.0
REL	"SPOAL7=SPOAL[7]"
INV_REL	"SPOAL[7]=SPOAL7"
FORMAT	"%14.3f"
TEXT	" "
END
T_NAME		SPOFFS7
TYPE	R32
CLASS	ACQU
SUBRANGE -1e38 1e38
REL	"SPOFFS7=SPOFFS[7]"
INV_REL	"SPOFFS[0]=SPOFFS0"
UNIT	"Hz"
FORMAT	"%14.2f Hz"
TEXT	" "
END
T_NAME		SPW7
TYPE	R32
CLASS	ACQU
REL	"SPW7=SPW[7]"
INV_REL	"SPW[7]=SPW7"
UNIT	"W"
FORMAT	"%14.8f W"
TEXT	"shaped pulse power SPW7"
END
NAME		GPNAM[1]
TEXT	" "
END
T_NAME		GPZ1
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ1=GPZ[1]"
INV_REL	"GPZ[1]=GPZ1"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[3]
TEXT	" "
END
T_NAME		GPZ3
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ3=GPZ[3]"
INV_REL	"GPZ[3]=GPZ3"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[4]
TEXT	" "
END
T_NAME		GPZ4
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ4=GPZ[4]"
INV_REL	"GPZ[4]=GPZ4"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[5]
TEXT	" "
END
T_NAME		GPZ5
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ5=GPZ[5]"
INV_REL	"GPZ[5]=GPZ5"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
NAME		GPNAM[6]
TEXT	" "
END
T_NAME		GPZ6
TYPE	R32
CLASS	ACQU
SUBRANGE -100.0 100.0
REL	"GPZ6=GPZ[6]"
INV_REL	"GPZ[6]=GPZ6"
UNIT	"%"
FORMAT	"%14.2f %"
TEXT	" "
END
T_NAME		P16
TYPE	R32
CLASS	ACQU
SUBRANGE 0.0 1.0e10
REL	"P16=P[16]"
INV_REL	"P[16]=P16"
UNIT	"usec"
FORMAT	"%14.2f usec"
TEXT	" "
END
HEADER		"======== F1 INDIRECT DIMENSION ========"
T_NAME		td1
		TYPE	I32
		CLASS	ACQU
		REL	"td1=256"
		INV_REL	"TD=TD"
		FORMAT	"%d"
		TEXT	"F1 Time domain size"
		NONEDIT
END
T_NAME		sw_F1
		TYPE	R32
		CLASS	ACQU
		REL	"sw_F1=239.997561"
		INV_REL	"SW=SW"
		FORMAT	"%f"
		TEXT	"F1 Sweep width [ppm]"
		NONEDIT
END
