! ----------------------------------------

! Create model and mesh

! ----------------------------------------

BLC4,0,0,Lx,Ly,Lz                        ! Create block volume from origin, with side of 5mm
VSEL,S,,,1                                            ! Select volume 1
VATT,1,,1,0                                           ! Set selected volume attributes to MAT=1,ET=1,Cartesian
MSHKEY,2                                           ! Mesh type: Mapped where possible, no smart size.
ALLSEL, ALL
ESIZE,,meshdivs                                              ! Mesh (element) size: no size set, meshdivs div's per boundary line
VMESH,ALL                                          ! Mesh all selected volumes



