"CL spectrum map header file"
"Width",70
"Height",70
"Pixels per spectrum",1600
"Data type","16-bit unsigned integer"
"Background data type","32-bit floating point"
"Raw, Background corrected or Reflectivity","Background corrected"
"Step size X (µm)",0.05
"Step size Y (µm)",0.05
"Spectrometer model","MS125"
"Grating (lines/mm)",600
"Centre wavelength (nm)",370
"Camera model","Andor Newton"
"Camera channels",1600
"Pixel pitch (mm)",0.016
"Channel binning",1
"Set temperature (°C)",-60
"Background averaging number",50
"Background averaging type","Mean"
"Background averaging standard deviations",2
"Electron multiplying on",#TRUE#
"Electron multiplying gain setting",150
"Exposure time (s)",0.5
"Horizontal read-out speed (MHz)",2.5
"Vertical read-out speed (µs)",19.35
