Methodology for repeats with 3Flex: The samples were degassed by heating to 300 °C under vacuum (below 1.3*10-2
mbar) for 5 h. After degassing, nitrogen was adsorbed at 77 K at increasing
partial pressures to determine the BET surface area and the pore volume