CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.5pl5/conf/instr/spect/uxnmr.info
Date         : Wed Feb 22 11:10:01 2017
Release      : TopSpin 3.5 pl 5
Installed in : C:/Bruker/TopSpin3.5pl5
Host         : CHPC-NMR500
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 3591 MHz with Hyperthreading)
User         : nmr
System       : Avance III 500 NMR spectrometer
1H-frequency : 500.13 MHz
Description  : Avance II+ 500
Location     : South Building 1
Bruker Order : GH000506
Configured in: CHPC-NMR500:C:/Bruker/TopSpin3.5pl5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/00420 ECL 02.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x3    AW  R  2.0 REC-1  AQS RXAD600 Z102117/205 ECL 02.00
     4   0x24 0x19   0x8    AD  S  1.0 SGU-1  AQS SGU/2 600 Z103081/00057 ECL 01.00 FPGA-Vs=AF
     5   0x25 0x19   0x8    AD  S  1.0 SGU-2  AQS SGU/2 600 Z103081/00043 ECL 01.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0016 W1345096/0016 ECL 0:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ: W1345096/0016 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0066 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0133 ECL 1

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20161026
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- 2HTX Amplifier: not available
- Lock: installed

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty01

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003461, SN=00466 from 20060307
    Module  2 : XBB19F 2HS
                PN=Z003505, SN=00500 from 20060404
    Module  3 : 2H
                PN=Z003472, SN=00479 from 20060509



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0016 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0016 at TCP/IP 149.236.99.253)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0016 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ W1345096/0016 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking


