For the experiments described in the paper two special fibre stages were needed. One with a two fixed platforms, anther with an extended fixed platform. Both of these have identical mechanisms to the standard stage. The code used to produce these stages is provided in these folders.

A number of accessories were used during the OpenSCAD code used to create these is in the accessories folder.

The Electronics and firmware for the motor driver board are in the same folder as the python package that drives the stage. `PythonPackages\openflexure_nano_motor_controller`

All files released under the CERN OHL license.