CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/AVII400/uxnmr.info
Date         : Tue Dec 22 12:08:47 2015
Release      : TOPSPIN Version 3.2-pl7
Installed in : C:/Bruker/TopSpin3.2
Host         : MARCUS
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : nmr
Description  : Avance-AV 400
Location     : University of St Andrews
System       : Avance-AV NMR spectrometer
1H-frequency : 400.13 MHz
Order Number : GH000306
Configured in: C:/Bruker/TopSpin3.2/conf/instr/AVII400

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU Z100977/00357 ECL 03.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 150604

Gcu: GCU3_SlowIF

AQS: connected to AVII400:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x3    AW  R  3.0 REC-1  AQS RXAD400 Z102116/408 ECL 03.00
     3   0x34  0x2   0x1        X  4.0 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x10   0x4    BH  S  6.2 SGU-1  AQS SGU400 Z003642/04151 ECL 6.2
     5   0x25 0x10   0x4    BH  S  6.2 SGU-2  AQS SGU400 Z003642/04136 ECL 6.2
     9   0x36  0x5     0        A  5.0 BLA-1  BLA2BB 150/60 20-400 W1345049/1630 ECL 5
    11   0x1a  0x9     0        C  3.0 ACB-S  ACB Standard
    23   0x20 0xc6     0        B  1.2 AQS/2  AQS/2 chassis
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS-Minirouter


Amplifiers (AQS configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        B      150    N         BLA2BB 150/60 20-400 W1345049/1630/-
   2      1         2        B       60    N         BLA2BB 150/60 20-400 W1345049/1630/-
   3      2         1       2H       20    N         BSMS 2HTX -/-/-



BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 20
- Shim System = BOSS1-SB
- 2HTX Amplifier: connected to router output 3
- Lock: installed

Bruker Automatic Changer: device connected to AVII400:/dev/tty08
- Capacity: 120 holders
- Firmware: 20040805
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to AVII400:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to AVII400:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 291.7%/77.7deg)
                 PN=Z003959, SN=00299 from 20060531
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 106.2%/-66.6deg)
                 PN=Z003959, SN=00299 from 20060531
    Module  3 : XBB19F 2HS
                 PN=Z003504, SN=00293 from 20060601


Frequency generation:
- F1: for SGU
- F2: for SGU



