CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Mon Jan 16 13:10:44 2017
Release      : TOPSPIN Version 3.2-pl7
Installed in : C:/Bruker/TopSpin3.2
Host         : ALEC
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 2533 MHz)
User         : nmr
Description  : Avance III 500
Location     : School of Chemistry, University of St Andrews 
System       : Avance III NMR spectrometer
1H-frequency : 500.13 MHz
Order Number : GH001711
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/02620 ECL 06.02
- TCP/IP address = 149.236.99.89
- Firmware Version = 150604
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  5.1 REC-1  AQS RXAD600 Z102117/1245 ECL 05.01
     3   0x34 0xc0   0x1        X  2.3 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.8 SGU-1  AQS SGU/2 600 Z103081/02835 ECL 02.08 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.8 SGU-2  AQS SGU/2 600 Z103081/02836 ECL 02.08 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0804 W1345096/0804 ECL 30:
- TCP/IP address = 149.236.99.254
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0804 ECL 30
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1320 ECL 2
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6054 ECL 50
- QNP-Accessory  : 1 X-input and 1 H-input
LTRX Z109889/00298 ECL 02.01:
- TCP/IP address = 149.236.99.21
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00298 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.21
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00298 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00640 ECL 03.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00736 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.21

Bruker Automatic Changer: device connected to 149.236.99.253:/dev/tty01
- Capacity: 60 holders
- Firmware: 20120928
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - BACS2_H15000-01_0242: at TCP/IP address 149.236.99.124


Prodigy Control Unit: LNP PRODIGY UNIT Z127349/323
- TCP/IP address   = 149.236.99.249

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 99.8%/0.2deg, reflection meter)
                 PN=Z103204, SN=00612 from 20141107
    Module  2 : XBB19F 2HS
                 PN=Z003505, SN=01089 from 20110922
    Module  3 : 2H
                 PN=Z003472, SN=00996 from 20110930


Frequency generation:
- F1: for SGU
- F2: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254)
SGU1 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254) amplifier X-300W uses blanking 1
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254) amplifier 2H-150W uses blanking 4
transmitter 2 (BSMS/2 LOCK TRANSCEIVER 500 Z109889/00298 at TCP/IP 149.236.99.21) amplifier 2H-5W needs no blanking

Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254 amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254 amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
BLAXH2H300/100/150 E 200-600MHZ W1345096/0804 at TCP/IP 149.236.99.254 amplifier 2H-150W at blanking 4 can be routed to switchbox output 5 (unknown)

