Klarite_001.fsp:
Material = Gold (Johnson & Christy); Max 6 Coeffs; Default Settings
Mesh Accuracy = 2; Standard Mesh Domain (No refinement region) - 0.015
Source Wavelength = 785 nm; Span = 500 nm
DFTMonitor = 785 nm; span = 1 nm; 9 frequency points

Klarite_002.fsp:
Material = Gold (Johnson & Christy); Max 6 Coeffs; Default Settings
Mesh Accuracy = 4; Standard Mesh Domain (No refinement region) - 0.0085 micron
Source Wavelength = 785 nm; Span = 500 nm
DFTMonitor = 785 nm; span = 1 nm; 9 frequency points

Klarite_003.fsp:
Material = Gold (Johnson & Christy); Max 6 Coeffs; Default Settings
Mesh Accuracy = 2; Refinement region accuracy = 6 - 0.005 micron
Source Wavelength = 785 nm; Span = 500 nm
DFTMonitor = 785 nm; span = 1 nm; 9 frequency points