This folder contains the calculations of electric fields and optical chirality 1 nm above the surface of an array of gold nanobars with varying length.

Simulations for different geometries are distinguished in the file name:
'I1' - array consisting of 400-nm gold bars,
'I2' - array consisting of 600-nm gold bars,
'I3' - array consisting of 800-nm gold bars,
'I4' - array consisting of 1000-nm gold bars.

Files with 'x' in the filename give the x-coordinates for which the simulation was performed in nanometers. Similarly for 'y'.

The simulations were performed for illumination with left circularly polarized light (LCP) and right circularly polarized light (RCP). The polarization of the incident light is specified in the filename as 'LCP' or 'RCP'.

The wavelength of illumination is also specified in the filename ('900nm' or '1100nm').

Files with 'modulus_E' in the filename contain the calculated modulus of electric field in multiples of the modulus of the incident electric field. The rows correspond to different y-coordinates and the columns to different x-coordinates.

Files with 'optical_chirality_results' in the filename contain the calculated optical chirality in multiples of the absolute value of the optical chirality of the incident light. The rows correspond to different y-coordinates and the columns to different x-coordinates.